This Mitsubishi ASA program is meant for 1987 and newer trucks and vehicles. It is the same type of program used at the dealer when searching for your parts when you ask the parts department
for parts. It has more details about parts then some of the manuals printed. I suaully start the program and type in "MM" in the vehicle name area and then in the following window I pick the truck.
For some reason the Mighty Max choice shows only 3 cylinder vehicles if your vehicle ID number does not work in the entry box and have to enter program using the "MM". Anyway, if you decide to
install the program and have any problems running it, just PM me at Bradmph in Mightyram50.net and I will get you running. Once you run the program once you will be familiar with the program's
format and it gets simple after that.



-Run the setup.exe file on your "disc".
 -During the install, you'll see a series of setup options, on the first one (if you see it), select the language of your choice (I didn't see this option but things came up in English so I was good). 
 -Next, you'll be asked for the location of the "Security Device"; check the box below the pic of a thumb drive titled "HASP HL". 
 -Next, select "Custom Install" and install it to the drive you want (C drive for most of us, I didn't have an option to specify a specific folder on the drive) and before clicking "Next" make sure "Single User" is selected. 
 -As things run their course, you'll be prompted for the 2nd disc; at this time, go and "mount" the B file or install the disc to which the B file was burned to. Then click to continue with the installation.
 -Once install is complete, it will ask you to finish but on the prompt it says to make sure to install security device before starting ASA; click "Finish"; you will get an error, click "Ok". 
 -Restart Windows.
 -When you start a new version of ASA for the first time a box will appear asking about connections, just click "Next" and you shouldn't see it again.
 -Enjoy your new version of ASA or install another starting over from the beginning. 




After installing the ASA program, you need to up to the latest version which I found was 1.4.0.2.
There is a RAR file in the folder you have named...ASA1402.rar  open this and take the file named ASA.exe
and place it into the C:\MMC\ASA\M50\PROG folder and overwrite the old file.
